You must config a user with privilege 15 if they use telnet on newer FW. We classified commands only for users with pri 15 could telnet to control switch totally in the newer FW. So be careful.





S9824-GS12M2#sh version
  S9824-GS12M2 Device, Compiled on May 16 20:30:00 2013
  sysLocation China
  CPU Mac 00:03:0f:3e:ba:fd
  Vlan MAC 00:03:0f:3e:ba:fc
  SoftWare Version 7.0.3.1(R0058.0002)
  BootRom Version 7.1.4
  HardWare Version 1.0.2
  CPLD Version N/A
  Serial No.:2ISWQ310E213790004

  All rights reserved
  Last reboot is warm reset.
  Uptime is 0 weeks, 0 days, 0 hours, 1 minutes
S9824-GS12M2#copy tftp://192.168.200.12/FoxGate_s9824_GS12M2_7.0.3.1(B0183.0033)_nos.img nos.img
Confirm to overwrite the existed destination file?  [Y/N]:y
Begin to receive file, please wait...
Get Img file size success, Img file size is:10195268(bytes).
#######################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################################
File transfer complete.
Recv total 10195268 bytes

Begin to write local file, please wait...

Write ok.
close tftp client.
S9824-GS12M2#reload
Process with reboot? [Y/N] ydcnos exit(SIGALRM)!
The system is going down NOW !!
Sending SIGTERM to all processes.
[1] + Done                       ./nos
Please stand by while rebooting the system.
Restarting system.




System is booting, please wait...



Bootrom version: 7.1.4

Creation date: Apr 25 2013 - 09:51:50

Testing RAM...
0x10000000 RAM OK.


Loading flash:/nos.img ...

Verifying Checksum ... OK
   Loading Kernel Image ...
Starting kernel in BE mode ...
Uncompressing Linux.............................................................................................................................................................................................................................................................................................................................................................. done, booting the kernel.


BusyBox v1.01 (2011.05.04-06:00+0000) Built-in shell (ash)
Enter 'help' for a list of built-in commands.

Current time is Sun Jan 01 00:00:00 2006

S9824-GS12M2 Series Switch Operating System
Software Version 7.0.3.1(B0183.0033)
Compiled Aug 28 16:52:50 2014

28 Ethernet/IEEE 802.3 interface(s)

Mac Addr 00-03-0f-3e-ba-fc

Recover config from file flash:/98.cfg
Loading startup-config ...
web server is on
%Jan 01 00:00:23 2006 %LINK-5-CHANGED: Interface Vlan1, changed state to UP
%Jan 01 00:00:23 2006 %LINK-5-CHANGED: Interface Ethernet1/0/1, changed state to UP
%Jan 01 00:00:23 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/1, changed state to DOWN
%Jan 01 00:00:24 2006 %LINK-5-CHANGED: Interface Ethernet1/0/2, changed state to UP
%Jan 01 00:00:24 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/2, changed state to DOWN
%Jan 01 00:00:24 2006 %LINK-5-CHANGED: Interface Ethernet1/0/3, changed state to UP
%Jan 01 00:00:24 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/3, changed state to DOWN
%Jan 01 00:00:24 2006 %LINK-5-CHANGED: Interface Ethernet1/0/4, changed state to UP
%Jan 01 00:00:24 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/4, changed state to DOWN
%Jan 01 00:00:24 2006 %LINK-5-CHANGED: Interface Ethernet1/0/5, changed state to UP
%Jan 01 00:00:24 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/5, changed state to DOWN
%Jan 01 00:00:24 2006 %LINK-5-CHANGED: Interface Ethernet1/0/6, changed state to UP
%Jan 01 00:00:24 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/6, changed state to DOWN
%Jan 01 00:00:25 2006 %LINK-5-CHANGED: Interface Ethernet1/0/7, changed state to UP
%Jan 01 00:00:25 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/7, changed state to DOWN
%Jan 01 00:00:25 2006 %LINK-5-CHANGED: Interface Ethernet1/0/8, changed state to UP
%Jan 01 00:00:25 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/8, changed state to DOWN
%Jan 01 00:00:25 2006 %LINK-5-CHANGED: Interface Ethernet1/0/9, changed state to UP
%Jan 01 00:00:25 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/9, changed state to DOWN
%Jan 01 00:00:25 2006 %LINK-5-CHANGED: Interface Ethernet1/0/10, changed state to UP
%Jan 01 00:00:25 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/10, changed state to DOWN
%Jan 01 00:00:25 2006 %LINK-5-CHANGED: Interface Ethernet1/0/11, changed state to UP
%Jan 01 00:00:25 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/11, changed state to DOWN
%Jan 01 00:00:25 2006 %LINK-5-CHANGED: Interface Ethernet1/0/12, changed state to UP
%Jan 01 00:00:25 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/12, changed state to DOWN
%Jan 01 00:00:26 2006 %LINK-5-CHANGED: Interface Ethernet1/0/13, changed state to UP
%Jan 01 00:00:26 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/13, changed state to DOWN
%Jan 01 00:00:26 2006 %LINK-5-CHANGED: Interface Ethernet1/0/14, changed state to UP
%Jan 01 00:00:26 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/14, changed state to DOWN
%Jan 01 00:00:26 2006 %LINK-5-CHANGED: Interface Ethernet1/0/15, changed state to UP
%Jan 01 00:00:26 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/15, changed state to DOWN
%Jan 01 00:00:26 2006 %LINK-5-CHANGED: Interface Ethernet1/0/16, changed state to UP
%Jan 01 00:00:26 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/16, changed state to DOWN
%Jan 01 00:00:26 2006 %LINK-5-CHANGED: Interface Ethernet1/0/17, changed state to UP
%Jan 01 00:00:26 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/17, changed state to DOWN
%Jan 01 00:00:27 2006 %LINK-5-CHANGED: Interface Ethernet1/0/18, changed state to UP
%Jan 01 00:00:27 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/18, changed state to DOWN
%Jan 01 00:00:27 2006 %LINK-5-CHANGED: Interface Ethernet1/0/19, changed state to UP
%Jan 01 00:00:27 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/19, changed state to DOWN
%Jan 01 00:00:27 2006 %LINK-5-CHANGED: Interface Ethernet1/0/20, changed state to UP
%Jan 01 00:00:27 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/20, changed state to DOWN
%Jan 01 00:00:27 2006 %LINK-5-CHANGED: Interface Ethernet1/0/21, changed state to UP
%Jan 01 00:00:27 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/21, changed state to DOWN
%Jan 01 00:00:27 2006 %LINK-5-CHANGED: Interface Ethernet1/0/22, changed state to UP
%Jan 01 00:00:27 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/22, changed state to DOWN
%Jan 01 00:00:27 2006 %LINK-5-CHANGED: Interface Ethernet1/0/23, changed state to UP
%Jan 01 00:00:27 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/23, changed state to DOWN
%Jan 01 00:00:28 2006 %LINK-5-CHANGED: Interface Ethernet1/0/24, changed state to UP
%Jan 01 00:00:28 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/24, changed state to DOWN
%Jan 01 00:00:28 2006 %LINK-5-CHANGED: Interface Ethernet1/0/25, changed state to UP
%Jan 01 00:00:28 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/25, changed state to DOWN
%Jan 01 00:00:28 2006 %LINK-5-CHANGED: Interface Ethernet1/0/26, changed state to UP
%Jan 01 00:00:28 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/26, changed state to DOWN
%Jan 01 00:00:28 2006 %LINK-5-CHANGED: Interface Ethernet1/0/27, changed state to UP
S9824-GS12M2#%Jan 01 00:00:28 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/27, changed state to DOWN
%Jan 01 00:00:28 2006 %LINK-5-CHANGED: Interface Ethernet1/0/28, changed state to UP
%Jan 01 00:00:28 2006 %LINEPROTO-5-UPDOWN: Line protocol on Interface Ethernet1/0/28, changed state to DOWN

S9824-GS12M2#sh version
  S9824-GS12M2 Device, Compiled on Aug 28 16:52:50 2014
  sysLocation China
  CPU Mac 00:03:0f:3e:ba:fd
  Vlan MAC 00:03:0f:3e:ba:fc
  SoftWare Version 7.0.3.1(B0183.0033)
  BootRom Version 7.1.4
  HardWare Version 1.0.2
  CPLD Version N/A
  Serial No.:2ISWQ310E213790004

  All rights reserved
  Last reboot is warm reset.
  Uptime is 0 weeks, 0 days, 0 hours, 0 minutes
S9824-GS12M2#sh ven
NAME            LEN          VALUE
------------    -----        ------------------------------
SwitchName      12           S9824-GS12M2
VersionPre      0
VendNameEn      12           FoxGate, Inc
VendNameBr      7            FoxGate
VendWWW         17           http://foxgate.ua
VendLocate      5            China
CopyRight       0
VendContact     0
WebLogo         2329
WebLogin        8821
WebFacebd       12701
WebBG           13495
WebLang         2            en
VendorOid       16           1.3.6.1.4.1.6339
DeviceOid       25           1.3.6.1.4.1.6339.1.1.2.39
KeyNeed         4            0
BaseMac         6            00 03 0f 03 00 00
CliStyle        3            0
HsrpNeed        4            0
DevType(ID)     4            170
ChassisCard     0
FileVersion     7            10.4.95
IMGPrefix       0
RomPrefix       0
HardWarePre     0
Prompt          0
UserName        0
PassWord        0
ManageIP        0

